**Part designation/ type**

|  |
| --- |
| This key designates and identifies all ebm-papst products and serves as part number: |

 R 2 E 190 -AO 26 -05

1 2 3 4 5 6 7

1. Type

A - axial fan

S - axial fan with guard grille

W - axial fan with wall ring

V - axial combination

R - centrifugal fan, single inlet

G - centrifugal blower, single inlet (with scroll housing)

B - centrifugal fan, dual inlet

D - centrifugal blower, dual inlet (with scroll housing)

K - centrifugal combination

M - motor

P - pumps

1. Number of poles (AC) / Number of cores (EC)

2-, 4-, 6-, 8- and 12-pole (Z =12) / 1- and 3-core

1. Motor type

D - 3-phase motor

E - single-phase motor with operating capacitor

G - EC motor

S - shaded-pole motor

Q - square shaded-pole motors

1. Impeller diameter in mm
2. Key for mechanical design
3. Key for electrical design
4. Key for mechanical variants